In this section, the extracted features from the LiDAR points are converted into a rasterized format. The resulting image has the same dimensions and resolution as the original aerial RGB image. Each band in the created image represents a specific feature of the LiDAR point clouds.